# Product Specification

|  |  |
| --- | --- |
| **Major parameter & Functions** | **Details** |
| Applicable Scene | Indoor |
| Operating System | Linux |
| Chip Model | CV1821 |
| Device Sorage | 128MB |
| Flash Space | 32MB |
| Sensor Model | SC3335 |
| Sensor Type | 1/2.7”CMOS |
| Maximum Pixels | 2304（H）\*1296（V）（16:9mode） |
| Focus Length | 3.9mm |
| Diagonal Angle Of View | 110° |
| Minimum Illumination | 0.1Lux (color mode)  0.001Lux (black and white mode)  0Lux (fill light ON) |
| Number Of Fill Light | 6 infrared lights |
| Night Vision Distance | 10 m |
| Frame Rate | Maximum 15 frames per second |
| TF Storage Card Port | Support 16-128G storage card |
| Voice Pickup | Built-in microphone,  3m of pickup distance |
| Loudspeaker | Support |
| Wired network | N/A |
| Camera Pan | horizontal 340°，horizontal 55° |
| Wi-Fi Standard | IEEE 802.11 b/g/n |
| Major Function | Human shape detection |
| Echo Suppression |
| Motion detection |
| Voice detection |
| Motion Tracking |
| Face recognition/capture |
| Voice intercom (full duplex) |
| Infrared night vision |
| Cloud playback /card playback |

|  |  |
| --- | --- |
| Product Photograph | |
| 正面图 | 后视图 |
| Front | Back |